|  |  |  |
| --- | --- | --- |
| Owner: | PHIN (if applicable): | Item Type: Item Type |
| Serial Number:  | Date Received: Click or tap to enter a date. | Date Removed from Service: Click or tap to enter a date. |
| **Date & Time of Inspection** | **Check (✓) if OK, (x) if problem identified, or N/A if not applicable to the item** | **Actions Taken if Problem Identified** |
| **Body of Item, Bands and Loops** | **Stitching: Body of Item, Bands and Loops** | **ID Label** | **Buckles and Clips** | **Miscella-neous** |
| No rips or holes, damage to material. | Velcro in good condition. | No bleach or heat damage. | No signs of fraying. | Stitching intact. | No broken/ frayed/ loose stitches. | ID label present and legible. | Buckle fastens securely. | No signs of damage to buckle/clips. | No knots at any part. | No pins, tape or other method to change the shape, shorten or lengthen the sling. | Item removed from service( Yes/No) | Supervisor Notified (Yes/No) | **Comments** | **Signature & Designation** |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

**Instructions**: See the *Pre-Use Mobility Equipment Inspection Guidelines* (CLI.6410.PL.007.SD.01) for detailed information about how to conduct mobility equipment inspections.